                                 CODE OF VIRGINIA

(FOR CONTINGENT EXPIRATION DATE, SEE ACTS 2025, CC. 91 AND 109, CL. 2) POSITION
OF SYSTEMS (§ 1-606)

The position of the Virginia coordinate systems shall be as marked on the ground
by triangulation or traverse stations established in conformity with the
standards of accuracy and specifications for first-order and second-order
geodetic surveying as prepared and published by the Federal Geodetic Control
Subcommittee of the Federal Geographic Data Committee of the U.S. Department of
Commerce. The geodetic position of stations defining the position of the
Virginia Coordinate System of 1927 shall have been rigidly adjusted on the North
American Datum of 1927, and the plane coordinates shall have been computed on
the Virginia Coordinate System of 1927. The geodetic position of stations
defining the position of the Virginia Coordinate System of 1983 shall have been
rigidly adjusted on the North American Datum of 1983, and the plane coordinates
shall have been computed on the Virginia Coordinate System of 1983. Any such
station may be used for establishing a survey connection with the Virginia
coordinate systems.

HISTORY: 1946, p. 168; Michie Suppl. 1946, § 2849(5); Code 1950, § 55-293;
1984, c. 726; 2019, c. 712.