                                 CODE OF VIRGINIA

CONSTRUCTIVE WEIGHT (§ 46.2-2164)

If no certified scale is available at origin, at any point enroute, or at
destination, a constructive weight based upon seven pounds per cubic foot of
properly loaded van space may be used.

HISTORY: 2001, c. 596.