                                 CODE OF VIRGINIA

 REQUIREMENTS OF RECOVERY WORK (§ 45.2-1139)

A. During recovery work and prior to entering any mine, each mine rescue team
conducting recovery work shall be properly informed of existing conditions by
the operator or his agent in charge.

B. Each mine rescue team performing rescue or recovery work with breathing
apparatus shall be provided with a backup team of equal strength, stationed at
each fresh air base.

C. For every two teams performing work underground, one six-member team shall be
stationed at the mine portal.

D. Two-way communication, life lines, or their equivalent shall be provided by
the fresh air base to each team, and no team member shall be permitted to
advance beyond such communication system.

E. A mine rescue team shall immediately return to the fresh air base if any team
member&#8217;s breathing apparatus malfunctions or the low-oxygen alarm
activates.

F. The Director may also assign rescue and recovery work to inspectors,
instructors, or other qualified employees of the Department as the Director
determines to be desirable.

HISTORY: 1997, c. 390, § 45.1-161.292:45; 2021, Sp. Sess. I, c. 387.